
I am using PIC16F1709 and I want to use pin RA2 as the DAC output. 
Flowcode8 does not allow me to set the DAC o/p pin. Default port A0. 
Looking at the form it appears it I set C code for DAC1CON0 = 10110000 (0XB0) this will enable pin RA2 and disable Pin AO. 
My question is my code correct in the attached Flowcode window and do I need to repeat the C block command during the program or will the Component Macro DAC_Output1 send the o/p to pin RA2?
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[Call ComponentMacro

DAC_Outputl :Enable(

[Call ComponentMacro

DAC_Outputl :SetOutput(DAC_OUT)

[Call ComponentMacro

ADC_1=pot_color_cap1:GetByte)

[Call ComponentMacro

ADC_2=pot_color_cap2:GetByte)

[Call ComponentMacro

ADC_3=pot_color_cap3:GetByte)

[Call ComponentMacro

ADC_4=pot_color_cap4:GetByte)
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ADC_ARRAY[1]=ADC_2





